{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["CDKOHSL","工程量清单"],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"CDKOHSL","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true}

{"sheet":"工程量清单","index":1,"n_rows":27,"n_cols":7,"rows_kept":27,"merged":[[0,0,0,6],[25,0,25,5],[26,0,26,6]]}
["G110线K555+000-K564+600段公路养护工程招标\n工程量清单"]
[{"$nulls":6},"货币单位：人民币元"]
["序号","项目名称","单位","工程量","最高限价单价\n(不含税)","投标单价      （不含税）","投标报价\n(不含税)"]
[1,"挖除沥青混凝土路面","m3",870.39,27,null,{"$f":"IF(F4>E4,\"报价无效\",D4*F4)","v":0}]
[2,"水泥稳定碎石基层","m3",1604.2,27,null,{"$f":"IF(F5>E5,\"报价无效\",D5*F5)","v":0}]
[3,"铣刨水稳","m3",7560.54,26,null,0]
[4,"铣刨沥青混凝土路面","m3",5369.328,26,null,0]
[5,"回填铣刨料","m3",3677.6,9,null,0]
[6,"水泥稳定级配碎石基层-厚200mm","m2",58924.8,46,null,0]
[7,"C20水泥混凝土基层","m3",1563.11,340,null,0]
[8,"水稳补基层","m3",763.5,212,null,0]
[9,"PC-2乳化沥青透层","m2",58924.8,4,null,0]
[10,"PCR改性乳化沥青粘层","m2",21026.8,1.8,null,0]
[11,"同步乳化沥青碎石封层","m2",58924.8,7.5,null,0]
[12,"中粒式改性沥青混合料路面-40mm","m2",78081.6,27,null,0]
[13,"中粒式改性沥青混合料路面-沥青混凝土过渡、找平层","m3",28.2,523,null,0]
[14,"砂砾培路肩","m3",1197.7,10.5,null,0]
[15,"现浇混凝土加固土路肩-C20混凝土","m3",147,500,null,0]
[16,"沥青路面拉毛","m2",50347.2,1.8,null,0]
[17,"路面灌缝","m",9017,7,null,0]
[18,"防撞墙栏杆涂漆","m",385,8,null,0]
[19,"防撞墙防腐涂层","m2",451,23,null,0]
[20,"沥青修补坑槽5cm","m2",1870,28,null,0]
[21,"热熔反光标线","m2",3073,36,null,0]
[22,"振动热熔反光标线","m2",1701,97,null,0]
["合计总金额 ",{"$nulls":5},{"$f":"SUM(G4:G25)","v":0}]
["注： 1、路面摊铺机械使用要求：福格勒2100-3L、天顺长城1860等机型。\n        2、水稳摊铺机械使用要求：天顺长城1660／1860、沃尔沃8820、徐工1253T/953T、三一C8系列等机型。\n        3、压路机系列使用要求：戴纳派克6200+宝马203+悍马138等机型。\n        4、其他要求：\n          （1）保险：施工单位给项目施工人员上雇主责任险（24小时）。\n          （2）特种作业人员必须持有特种人员证书，特种设备操作证。\n          （3）资金拨付情况由业主拨款后再向乙方支付。\n     5、包含施工、材料、机械、安全布控及施工过程中产生的一切费用（最终结算以实际面积为准,不含沥青）"]